1. The circuit works by first going through a SIP resistor, into a DIP switch array, three of which go into a 74LS138 (3-to-8 Decoder), to convert three binary bits into 8 different positions. Then,